config
https-server vrf default
ssh server vrf default
hostname NET-SW04
snmp-server system-contact Jan Baulig
snmp-server system-location Serverraum Neu
ip dns domain-name aps.local
ip dns server-address 10.102.1.1
ip dns host Sophos 10.102.1.1
ntp enable
ntp server 10.102.1.1 iburst version 4 prefer
ntp server 0.de.pool.ntp.org iburst version 4
ntp server 1.de.pool.ntp.org iburst version 4
clock timezone europe/berlin
https-server rest firmware-site-distribution
spanning-tree mode rpvst
spanning-tree pathcost-type long
loop-protect re-enable-timer 30
banner motd #
                                                   Hostname: NET-SW04
                                            System Location: Serverraum Neu
                                             System Contact: Jan Baulig
#
vlan 1
exit
vlan 9
description Drucker
name VLAN_9_Drucker
exit
vlan 10
description Server
name VLAN_10_Server
exit
vlan 20
description Client
name VLAN_20_Client
exit
vlan 66
description WLAN
name VLAN_66_WLAN
exit
vlan 97
description Network-MGMT
name VLAN_97_Network-MGMT
exit
vlan 1820
description Antares Apotheke APS
name VLAN_1820_Antares_Apotheke_APS
exit
vlan 2012
description Gastnetz_LAN
name VLAN_2012_Gastnetz_LAN
exit
interface vlan 1
description Admin Interface
loop-protect
no ip dhcp
no shutdown
ip address 192.168.9.5/24
ip route 0.0.0.0/0 10.220.1.1
config
interface vlan 97
description Management Interface
loop-protect
no shutdown
ip address 10.220.1.86/24
ip route 0.0.0.0/0 10.220.1.1
config
interface 1/1/1
description Admin Port
vlan trunk native 1
vlan trunk allow 1,9,20,97
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree root-guard
spanning-tree tcn-guard
spanning-tree rpvst-guard
no shutdown
exit
interface 1/1/2-1/1/47
vlan trunk native 20
vlan trunk allow 9,20
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree root-guard
spanning-tree tcn-guard
spanning-tree rpvst-guard
no shutdown
exit
interface 1/1/22
vlan trunk native 20
vlan trunk allow 10,20
description NET-LOGGER01
exit
interface 1/1/24
vlan access 9
description Drucker Enz
exit
interface 1/1/39
vlan access 9
description Drucker Belt
exit
interface 1/1/45
vlan access 97
description NET-COL01
exit
interface 1/1/48-1/1/52
vlan trunk native 1
vlan trunk allow all
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree rpvst-guard
no shutdown
exit
client track ip
client track ip all-vlan
interface 1/1/3
description Uplink NET-AP03 Apotheke 02
exit
interface 1/1/4
description Uplink NET-AP03 Apotheke 01
exit
interface 1/1/41
vlan access 20
description NET-DECT01
exit
interface 1/1/49
description Uplink NET-SW01-Core Port 18
exit
wr mem
copy running-config startup-config
copy running-config checkpoint Config_27102025


