config
https-server vrf default
ssh server vrf default
hostname NET-SW19
snmp-server system-contact Jan Baulig
snmp-server system-location Serverschrank Stade
ip dns domain-name aps.local
ip dns server-address 10.102.1.1
ip dns host Sophos 10.102.1.1
ntp enable
ntp server 10.102.1.1 iburst version 4 prefer
ntp server 0.de.pool.ntp.org iburst version 4
ntp server 1.de.pool.ntp.org iburst version 4
clock timezone europe/berlin
spanning-tree mode rpvst
spanning-tree pathcost-type long
banner motd #
                                                    Hostname: NET-SW19
                                             System Location: Serverschrank Stade
                                              System Contact: Jan Baulig
#
vlan 1
exit
vlan 1820
description Antares Apotheke APS
name VLAN_1820_Antares_Apotheke_APS
exit
vlan 1830
description APS-WLAN-Scanner
name VLAN_1830_APS-WLAN-Scanner
exit
vlan 2012
description Gastnetz_LAN
name VLAN_2012_Gastnetz_LAN
exit
interface vlan 1
description Admin Interface
no ip dhcp
no shutdown
config
interface vlan 97
description Management Interface
no shutdown
ip address 10.220.1.99/24
ip route 0.0.0.0/0 10.220.1.1
config
interface 1/1/1
vlan trunk native 20
vlan trunk allow 9,20,97
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree root-guard
spanning-tree tcn-guard
spanning-tree rpvst-guard
no shutdown
description Admin Port
exit
interface 1/1/2-1/1/48
vlan trunk native 20
vlan trunk allow 9,20
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree root-guard
spanning-tree tcn-guard
spanning-tree rpvst-guard
no shutdown
exit
interface 1/1/49-1/1/52
vlan trunk native 1
vlan trunk allow all
loop-protect
spanning-tree loop-guard
spanning-tree bpdu-guard
spanning-tree rpvst-guard
no shutdown
exit
client track ip
client track ip all-vlan
interface 1/1/49
wr mem
copy running-config startup-config
copy running-config checkpoint Config_04112025
end
exit


